|  |  |
| --- | --- |
| **Computer Architectures**  **02LSEOV** | Delivery date:  **By 2:00 AM on October, 16 2024** |
| **Laboratory**  **2** | The expected delivery of lab\_02.zip must include:   * **program\_1.s** * This file, filled with information and possibly compiled in a pdf format. |

Please configure the WinMIPS64 simulator with the *Initial Configuration* provided below c):

* *Integer ALU: 1 clock cycle*
* *Data memory: 1 clock cycle*
* Code address bus: 12
* Data address bus: 12
* FP arithmetic unit: pipelined, 4 clock cycles
* FP multiplier unit: pipelined, 6 clock cycles
* FP divider unit: not pipelined, 30 clock cycles

1. Write an assembly program (**program\_1.s**) for the *WinMIPS64* architecture described before being able to implement the following high-level code:

for (i = 31; i >= 0; i--){

v4[i] = v1[i]\*v1[i] – v2[i];

v5[i] = v4[i]/v3[i] – v2[i];

v6[i] = (v4[i]-v1[i])\*v5[i];

}

Assume that the vectors v1[], v2[], and v3[] have been previously allocated in memory and contain 32 double-precision **floating-point values;** also assume that v3[] doesnot contain 0 values. Additionally, the vectors v4[], v5[], v6[] are empty vectors also allocated in memory.

**Calculate** the data memory footprint of your program:

|  |  |
| --- | --- |
| Data | Number of bytes |
| V1 | 256 |
| V2 | 256 |
| V3 | 256 |
| V4 | 256 |
| V5 | 256 |
| V6 | 256 |
| Total | 1536 |

Are there any issues? Yes, where and why? No? Do you need to change something?

|  |
| --- |
| Your answer:  Con la configurazione indicata non si hanno problemi, ma se si fosse utilizzato un databus minore come quello nelle impostazioni di default di winmips allora non si sarebbe potuto eseguire il programma correttamente. |

ATTENTION: WinMIPS64 has a limitation regarding the maximum length of the string when declaring a vector. It is therefore recommended to split the elements of the vectors into multiple lines: this also increases readability.

Example: my\_fancy\_vector: .byte 8, 12 ,2, 9

.byte 49,77, 28

.byte ……

* + - Calculate the CPU performance equation (CPU time) of the above program by assuming a clock frequency of 15 MHz:

By definition:

* + - * CPI is equal to the number of clock cycles required by the related functional unit to execute the instruction (EX stage).
      * IC*i* is the number of times an instruction is repeated in the referenced source code.
    - Recalculate the CPU performance equation assuming that you can triple the speed by just one unit of your choice between the FP multiplier or the FP divider:
      * FP multiplier unit: 6 🡪 2 clock cycles

*or*

* + - * FP divider unit: 30 🡪 10 clock cycles

Table 1: CPU time by hand

|  |  |  |  |
| --- | --- | --- | --- |
|  | Initial CPU time (a) | CPU time  (b – MUL speeded up) | CPU time  (b – DIV speeded up) |
| program\_1.s | 0.145ms | 0.128ms | 0.103ms |

* + - Using the simulator, calculate the CPU time again and fill in the following table:

Table 2: CPU time using the simulator

|  |  |  |  |
| --- | --- | --- | --- |
|  | Initial CPU time (a) | CPU time  (b – MUL speeded up) | CPU time  (b – DIV speeded up) |
| program\_1.s | 0.186ms | 0.169ms | 0.143ms |

Are there any differences? If so, where and why? If not, please provide some comments in the box below:

|  |
| --- |
| Your answer: I due risultati sono diversi perchè nel calcolo a mano si tengono solo in considerazioni i cicli di excute relativi a ciascuna istruzione. Invece nel simulatore si considerano gli stalli e tutti gli altri stati di un istruzione. |

* + - Using the simulator and the *Initial Configuration*, enable the Forwarding option and compute how many clock cycles the program takes to execute.

Table 3: forwarding enabled

|  |  |  |
| --- | --- | --- |
|  | Number of clock cycles | IPC (Instructions Per Clock) |
| program\_1.s | 2280 | 0.296 |

Enable one at a time the *optimization features* that were initially disabled and collect statistics to fill the following table (fill all required data in the table before exporting this file to pdf format to be delivered).

Table 4: **Program performance for different processor configurations**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Program | Forwarding | | Branch Target Buffer | | Delay Slot | | Forwarding + Branch Target Buffer | |
|  | IPC | CC | IPC | CC | IPC | CC | IPC | CC |
| program\_1.s | 0.296 | 2280 | 0.244 2766 | | 0.274 95 | | 0.300 2254 | |

1. Using the WinMIPS64 simulator, validate experimentally the Amdahl’s law, defined as follows:



1. Using the program developed before: **program\_1.s**
2. Modify the processor architectural parameters related to multicycle instructions (Menu🡪Configure🡪Architecture) in the following way:
   * + - 1. Configuration 1

Starting from the *Initial Configuration*, change the FP addition latency to 3

* + - * 1. Configuration 2

Starting from the *Initial Configuration*, change the FP multiplier latency to 4

* + - * 1. Configuration 3

Starting from the *Initial Configuration*, change the FP division latency to 10

Compute both manually (using the Amdahl’s Law) and with the simulator the speed-up for any one of the previous processor configurations. Compare the obtained results and complete the following table.

Table 5: **program\_1.s speed-up computed by hand and by simulation**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Proc. Config.**    **Speed-up comp.** | Initial config.  [c.c.] | Config. 1 | Config. 2 | Config. 3 |
| **By hand** | 2180 | 1.046 | 1.062 | 1.415 |
| **By simulation** | 2792 | 1.035 | 1.045 | 1.297 |